 -- Copyright (C) 1991-2013 Altera Corporation
 -- Your use of Altera Corporation's design tools, logic functions 
 -- and other software and tools, and its AMPP partner logic 
 -- functions, and any output files from any of the foregoing 
 -- (including device programming or simulation files), and any 
 -- associated documentation or information are expressly subject 
 -- to the terms and conditions of the Altera Program License 
 -- Subscription Agreement, Altera MegaCore Function License 
 -- Agreement, or other applicable license agreement, including, 
 -- without limitation, that your use is for the sole purpose of 
 -- programming logic devices manufactured by Altera and sold by 
 -- Altera or its authorized distributors.  Please refer to the 
 -- applicable agreement for further details.
 -- 
 -- This is a Quartus II output file. It is for reporting purposes only, and is
 -- not intended for use as a Quartus II input file. This file cannot be used
 -- to make Quartus II pin assignments - for instructions on how to make pin
 -- assignments, please see Quartus II help.
 ---------------------------------------------------------------------------------



 ---------------------------------------------------------------------------------
 -- NC            : No Connect. This pin has no internal connection to the device.
 -- DNU           : Do Not Use. This pin MUST NOT be connected.
 -- VCCINT        : Dedicated power pin, which MUST be connected to VCC  (1.2V).
 -- VCCIO         : Dedicated power pin, which MUST be connected to VCC
 --                 of its bank.
 --					Bank 1:		3.3V
 --					Bank 2:		3.3V
 --					Bank 3:		3.3V
 --					Bank 4:		3.3V
 --					Bank 5:		3.3V
 --					Bank 6:		3.3V
 --					Bank 7:		3.3V
 --					Bank 8:		3.3V
 -- GND           : Dedicated ground pin. Dedicated GND pins MUST be connected to GND.
 --					It can also be used to report unused dedicated pins. The connection
 --					on the board for unused dedicated pins depends on whether this will
 --					be used in a future design. One example is device migration. When
 --					using device migration, refer to the device pin-tables. If it is a
 --					GND pin in the pin table or if it will not be used in a future design
 --					for another purpose the it MUST be connected to GND. If it is an unused
 --					dedicated pin, then it can be connected to a valid signal on the board
 --					(low, high, or toggling) if that signal is required for a different
 --					revision of the design.
 -- GND+          : Unused input pin. It can also be used to report unused dual-purpose pins.
 --					This pin should be connected to GND. It may also be connected  to a
 --					valid signal  on the board  (low, high, or toggling)  if that signal
 --					is required for a different revision of the design.
 -- GND*          : Unused  I/O  pin. Connect each pin marked GND* directly to GND
 --           	    or leave it unconnected.
 -- RESERVED      : Unused I/O pin, which MUST be left unconnected.
 -- RESERVED_INPUT    : Pin is tri-stated and should be connected to the board.
 -- RESERVED_INPUT_WITH_WEAK_PULLUP    : Pin is tri-stated with internal weak pull-up resistor.
 -- RESERVED_INPUT_WITH_BUS_HOLD       : Pin is tri-stated with bus-hold circuitry.
 -- RESERVED_OUTPUT_DRIVEN_HIGH        : Pin is output driven high.
 ---------------------------------------------------------------------------------



 ---------------------------------------------------------------------------------
 -- Pin directions (input, output or bidir) are based on device operating in user mode.
 ---------------------------------------------------------------------------------

Quartus II 32-bit Version 13.1.0 Build 162 10/23/2013 SJ Web Edition
CHIP  "spectrum"  ASSIGNED TO AN: EP4CE22F17C6

Pin Name/Usage               : Location  : Dir.   : I/O Standard      : Voltage : I/O Bank  : User Assignment
-------------------------------------------------------------------------------------------------------------
VCCIO8                       : A1        : power  :                   : 3.3V    : 8         :                
RESERVED_INPUT_WITH_WEAK_PULLUP : A2        :        :                   :         : 8         :                
RESERVED_INPUT_WITH_WEAK_PULLUP : A3        :        :                   :         : 8         :                
RESERVED_INPUT_WITH_WEAK_PULLUP : A4        :        :                   :         : 8         :                
RESERVED_INPUT_WITH_WEAK_PULLUP : A5        :        :                   :         : 8         :                
buzzer_out                   : A6        : output : 3.3-V LVTTL       :         : 8         : Y              
AUD_XCK                      : A7        : output : 3.3-V LVTTL       :         : 8         : Y              
GND+                         : A8        :        :                   :         : 8         :                
GND+                         : A9        :        :                   :         : 7         :                
RESERVED_INPUT_WITH_WEAK_PULLUP : A10       :        :                   :         : 7         :                
LED[3]                       : A11       : output : 3.3-V LVTTL       :         : 7         : Y              
VGA_B[2]                     : A12       : output : 3.3-V LVTTL       :         : 7         : Y              
LED[1]                       : A13       : output : 3.3-V LVTTL       :         : 7         : Y              
RESERVED_INPUT_WITH_WEAK_PULLUP : A14       :        :                   :         : 7         :                
LED[0]                       : A15       : output : 3.3-V LVTTL       :         : 7         : Y              
VCCIO7                       : A16       : power  :                   : 3.3V    : 7         :                
LED[6]                       : B1        : output : 3.3-V LVTTL       :         : 1         : Y              
GND                          : B2        : gnd    :                   :         :           :                
RESERVED_INPUT_WITH_WEAK_PULLUP : B3        :        :                   :         : 8         :                
RESERVED_INPUT_WITH_WEAK_PULLUP : B4        :        :                   :         : 8         :                
RESERVED_INPUT_WITH_WEAK_PULLUP : B5        :        :                   :         : 8         :                
raw_loader_in                : B6        : input  : 3.3-V LVTTL       :         : 8         : Y              
PS2_DAT                      : B7        : input  : 3.3-V LVTTL       :         : 8         : Y              
GND+                         : B8        :        :                   :         : 8         :                
SW[2]                        : B9        : input  : 3.3-V LVTTL       :         : 7         : Y              
RESERVED_INPUT_WITH_WEAK_PULLUP : B10       :        :                   :         : 7         :                
VGA_B[1]                     : B11       : output : 3.3-V LVTTL       :         : 7         : Y              
VGA_VS                       : B12       : output : 3.3-V LVTTL       :         : 7         : Y              
LED[2]                       : B13       : output : 3.3-V LVTTL       :         : 7         : Y              
RESERVED_INPUT_WITH_WEAK_PULLUP : B14       :        :                   :         : 7         :                
GND                          : B15       : gnd    :                   :         :           :                
RESERVED_INPUT_WITH_WEAK_PULLUP : B16       :        :                   :         : 6         :                
~ALTERA_ASDO_DATA1~ / RESERVED_INPUT_WITH_WEAK_PULLUP : C1        : input  : 3.3-V LVTTL       :         : 1         : N              
DRAM_WE_N                    : C2        : output : 3.3-V LVTTL       :         : 1         : Y              
RESERVED_INPUT_WITH_WEAK_PULLUP : C3        :        :                   :         : 8         :                
VCCIO8                       : C4        : power  :                   : 3.3V    : 8         :                
GND                          : C5        : gnd    :                   :         :           :                
AUD_DACLRCK                  : C6        : output : 3.3-V LVTTL       :         : 8         : Y              
VCCIO8                       : C7        : power  :                   : 3.3V    : 8         :                
AUD_DACDAT                   : C8        : output : 3.3-V LVTTL       :         : 8         : Y              
VGA_G[0]                     : C9        : output : 3.3-V LVTTL       :         : 7         : Y              
VCCIO7                       : C10       : power  :                   : 3.3V    : 7         :                
VGA_B[0]                     : C11       : output : 3.3-V LVTTL       :         : 7         : Y              
GND                          : C12       : gnd    :                   :         :           :                
VCCIO7                       : C13       : power  :                   : 3.3V    : 7         :                
RESERVED_INPUT_WITH_WEAK_PULLUP : C14       :        :                   :         : 7         :                
RESERVED_INPUT_WITH_WEAK_PULLUP : C15       :        :                   :         : 6         :                
RESERVED_INPUT_WITH_WEAK_PULLUP : C16       :        :                   :         : 6         :                
LED[4]                       : D1        : output : 3.3-V LVTTL       :         : 1         : Y              
~ALTERA_FLASH_nCE_nCSO~ / RESERVED_INPUT_WITH_WEAK_PULLUP : D2        : input  : 3.3-V LVTTL       :         : 1         : N              
RESERVED_INPUT_WITH_WEAK_PULLUP : D3        :        :                   :         : 8         :                
VCCD_PLL3                    : D4        : power  :                   : 1.2V    :           :                
RESERVED_INPUT_WITH_WEAK_PULLUP : D5        :        :                   :         : 8         :                
PS2_CLK                      : D6        : input  : 3.3-V LVTTL       :         : 8         : Y              
GND                          : D7        : gnd    :                   :         :           :                
AUD_ADCDAT                   : D8        : input  : 3.3-V LVTTL       :         : 8         : Y              
VGA_G[1]                     : D9        : output : 3.3-V LVTTL       :         : 7         : Y              
GND                          : D10       : gnd    :                   :         :           :                
VGA_B[3]                     : D11       : output : 3.3-V LVTTL       :         : 7         : Y              
VGA_HS                       : D12       : output : 3.3-V LVTTL       :         : 7         : Y              
VCCD_PLL2                    : D13       : power  :                   : 1.2V    :           :                
RESERVED_INPUT_WITH_WEAK_PULLUP : D14       :        :                   :         : 7         :                
RESERVED_INPUT_WITH_WEAK_PULLUP : D15       :        :                   :         : 6         :                
RESERVED_INPUT_WITH_WEAK_PULLUP : D16       :        :                   :         : 6         :                
KEY[1]                       : E1        : input  : 3.3-V LVTTL       :         : 1         : Y              
GND                          : E2        : gnd    :                   :         :           :                
VCCIO1                       : E3        : power  :                   : 3.3V    : 1         :                
GND                          : E4        : gnd    :                   :         :           :                
GNDA3                        : E5        : gnd    :                   :         :           :                
AUD_BCLK                     : E6        : output : 3.3-V LVTTL       :         : 8         : Y              
AUD_ADCLRCK                  : E7        : output : 3.3-V LVTTL       :         : 8         : Y              
VGA_R[0]                     : E8        : output : 3.3-V LVTTL       :         : 8         : Y              
VGA_R[3]                     : E9        : output : 3.3-V LVTTL       :         : 7         : Y              
VGA_G[3]                     : E10       : output : 3.3-V LVTTL       :         : 7         : Y              
VGA_G[2]                     : E11       : output : 3.3-V LVTTL       :         : 7         : Y              
GNDA2                        : E12       : gnd    :                   :         :           :                
GND                          : E13       : gnd    :                   :         :           :                
VCCIO6                       : E14       : power  :                   : 3.3V    : 6         :                
GND+                         : E15       :        :                   :         : 6         :                
GND+                         : E16       :        :                   :         : 6         :                
I2C_SDAT                     : F1        : bidir  : 3.3-V LVTTL       :         : 1         : Y              
I2C_SCLK                     : F2        : bidir  : 3.3-V LVTTL       :         : 1         : Y              
LED[5]                       : F3        : output : 3.3-V LVTTL       :         : 1         : Y              
nSTATUS                      : F4        :        :                   :         : 1         :                
VCCA3                        : F5        : power  :                   : 2.5V    :           :                
GND                          : F6        : gnd    :                   :         :           :                
VCCINT                       : F7        : power  :                   : 1.2V    :           :                
VGA_R[1]                     : F8        : output : 3.3-V LVTTL       :         : 8         : Y              
VGA_R[2]                     : F9        : output : 3.3-V LVTTL       :         : 7         : Y              
GND                          : F10       : gnd    :                   :         :           :                
VCCINT                       : F11       : power  :                   : 1.2V    :           :                
VCCA2                        : F12       : power  :                   : 2.5V    :           :                
GPIO_1[0]                    : F13       : output : 3.3-V LVTTL       :         : 6         : Y              
RESERVED_INPUT_WITH_WEAK_PULLUP : F14       :        :                   :         : 6         :                
RESERVED_INPUT_WITH_WEAK_PULLUP : F15       :        :                   :         : 6         :                
~ALTERA_nCEO~ / RESERVED_OUTPUT_OPEN_DRAIN : F16       : output : 3.3-V LVTTL       :         : 6         : N              
DRAM_DQ[1]                   : G1        : bidir  : 3.3-V LVTTL       :         : 1         : Y              
DRAM_DQ[0]                   : G2        : bidir  : 3.3-V LVTTL       :         : 1         : Y              
VCCIO1                       : G3        : power  :                   : 3.3V    : 1         :                
GND                          : G4        : gnd    :                   :         :           :                
RESERVED_INPUT_WITH_WEAK_PULLUP : G5        :        :                   :         : 1         :                
VCCINT                       : G6        : power  :                   : 1.2V    :           :                
VCCINT                       : G7        : power  :                   : 1.2V    :           :                
VCCINT                       : G8        : power  :                   : 1.2V    :           :                
VCCINT                       : G9        : power  :                   : 1.2V    :           :                
VCCINT                       : G10       : power  :                   : 1.2V    :           :                
GND                          : G11       : gnd    :                   :         :           :                
MSEL2                        : G12       :        :                   :         : 6         :                
GND                          : G13       : gnd    :                   :         :           :                
VCCIO6                       : G14       : power  :                   : 3.3V    : 6         :                
RESERVED_INPUT_WITH_WEAK_PULLUP : G15       :        :                   :         : 6         :                
RESERVED_INPUT_WITH_WEAK_PULLUP : G16       :        :                   :         : 6         :                
~ALTERA_DCLK~                : H1        : output : 3.3-V LVTTL       :         : 1         : N              
~ALTERA_DATA0~ / RESERVED_INPUT_WITH_WEAK_PULLUP : H2        : input  : 3.3-V LVTTL       :         : 1         : N              
TCK                          : H3        : input  :                   :         : 1         :                
TDI                          : H4        : input  :                   :         : 1         :                
nCONFIG                      : H5        :        :                   :         : 1         :                
VCCINT                       : H6        : power  :                   : 1.2V    :           :                
GND                          : H7        : gnd    :                   :         :           :                
GND                          : H8        : gnd    :                   :         :           :                
GND                          : H9        : gnd    :                   :         :           :                
GND                          : H10       : gnd    :                   :         :           :                
VCCINT                       : H11       : power  :                   : 1.2V    :           :                
MSEL1                        : H12       :        :                   :         : 6         :                
MSEL0                        : H13       :        :                   :         : 6         :                
CONF_DONE                    : H14       :        :                   :         : 6         :                
GND                          : H15       : gnd    :                   :         :           :                
GND                          : H16       : gnd    :                   :         :           :                
DRAM_DQ[6]                   : J1        : bidir  : 3.3-V LVTTL       :         : 2         : Y              
DRAM_DQ[5]                   : J2        : bidir  : 3.3-V LVTTL       :         : 2         : Y              
nCE                          : J3        :        :                   :         : 1         :                
TDO                          : J4        : output :                   :         : 1         :                
TMS                          : J5        : input  :                   :         : 1         :                
VCCINT                       : J6        : power  :                   : 1.2V    :           :                
GND                          : J7        : gnd    :                   :         :           :                
GND                          : J8        : gnd    :                   :         :           :                
GND                          : J9        : gnd    :                   :         :           :                
GND                          : J10       : gnd    :                   :         :           :                
GND                          : J11       : gnd    :                   :         :           :                
VCCINT                       : J12       : power  :                   : 1.2V    :           :                
GPIO_1[32]                   : J13       : output : 3.3-V LVTTL       :         : 5         : Y              
GPIO_1[33]                   : J14       : output : 3.3-V LVTTL       :         : 5         : Y              
KEY[0]                       : J15       : input  : 3.3-V LVTTL       :         : 5         : Y              
GPIO_1[30]                   : J16       : output : 3.3-V LVTTL       :         : 5         : Y              
DRAM_DQ[15]                  : K1        : bidir  : 3.3-V LVTTL       :         : 2         : Y              
DRAM_DQ[4]                   : K2        : bidir  : 3.3-V LVTTL       :         : 2         : Y              
VCCIO2                       : K3        : power  :                   : 3.3V    : 2         :                
GND                          : K4        : gnd    :                   :         :           :                
DRAM_DQ[3]                   : K5        : bidir  : 3.3-V LVTTL       :         : 2         : Y              
GND                          : K6        : gnd    :                   :         :           :                
VCCINT                       : K7        : power  :                   : 1.2V    :           :                
GND                          : K8        : gnd    :                   :         :           :                
VCCINT                       : K9        : power  :                   : 1.2V    :           :                
VCCINT                       : K10       : power  :                   : 1.2V    :           :                
VCCINT                       : K11       : power  :                   : 1.2V    :           :                
GND                          : K12       : gnd    :                   :         :           :                
GND                          : K13       : gnd    :                   :         :           :                
VCCIO5                       : K14       : power  :                   : 3.3V    : 5         :                
GPIO_1[31]                   : K15       : output : 3.3-V LVTTL       :         : 5         : Y              
GPIO_1[17]                   : K16       : output : 3.3-V LVTTL       :         : 5         : Y              
DRAM_CAS_N                   : L1        : output : 3.3-V LVTTL       :         : 2         : Y              
DRAM_RAS_N                   : L2        : output : 3.3-V LVTTL       :         : 2         : Y              
LED[7]                       : L3        : output : 3.3-V LVTTL       :         : 2         : Y              
DRAM_ADDR[12]                : L4        : output : 3.3-V LVTTL       :         : 2         : Y              
VCCA1                        : L5        : power  :                   : 2.5V    :           :                
VCCINT                       : L6        : power  :                   : 1.2V    :           :                
DRAM_CKE                     : L7        : output : 3.3-V LVTTL       :         : 3         : Y              
DRAM_DQ[2]                   : L8        : bidir  : 3.3-V LVTTL       :         : 3         : Y              
GND                          : L9        : gnd    :                   :         :           :                
GND                          : L10       : gnd    :                   :         :           :                
GND                          : L11       : gnd    :                   :         :           :                
VCCA4                        : L12       : power  :                   : 2.5V    :           :                
GPIO_1[29]                   : L13       : output : 3.3-V LVTTL       :         : 5         : Y              
GPIO_1[26]                   : L14       : output : 3.3-V LVTTL       :         : 5         : Y              
GPIO_1[19]                   : L15       : output : 3.3-V LVTTL       :         : 5         : Y              
GPIO_1[16]                   : L16       : output : 3.3-V LVTTL       :         : 5         : Y              
SW[0]                        : M1        : input  : 3.3-V LVTTL       :         : 2         : Y              
GND+                         : M2        :        :                   :         : 2         :                
VCCIO2                       : M3        : power  :                   : 3.3V    : 2         :                
GND                          : M4        : gnd    :                   :         :           :                
GNDA1                        : M5        : gnd    :                   :         :           :                
DRAM_BA[1]                   : M6        : output : 3.3-V LVTTL       :         : 3         : Y              
DRAM_BA[0]                   : M7        : output : 3.3-V LVTTL       :         : 3         : Y              
DRAM_ADDR[3]                 : M8        : output : 3.3-V LVTTL       :         : 3         : Y              
VCCINT                       : M9        : power  :                   : 1.2V    :           :                
GPIO_1[28]                   : M10       : output : 3.3-V LVTTL       :         : 4         : Y              
VCCINT                       : M11       : power  :                   : 1.2V    :           :                
GNDA4                        : M12       : gnd    :                   :         :           :                
GND                          : M13       : gnd    :                   :         :           :                
VCCIO5                       : M14       : power  :                   : 3.3V    : 5         :                
SW[3]                        : M15       : input  : 3.3-V LVTTL       :         : 5         : Y              
GND+                         : M16       :        :                   :         : 5         :                
DRAM_ADDR[11]                : N1        : output : 3.3-V LVTTL       :         : 2         : Y              
DRAM_ADDR[10]                : N2        : output : 3.3-V LVTTL       :         : 2         : Y              
DRAM_DQ[14]                  : N3        : bidir  : 3.3-V LVTTL       :         : 3         : Y              
VCCD_PLL1                    : N4        : power  :                   : 1.2V    :           :                
DRAM_ADDR[1]                 : N5        : output : 3.3-V LVTTL       :         : 3         : Y              
DRAM_ADDR[2]                 : N6        : output : 3.3-V LVTTL       :         : 3         : Y              
GND                          : N7        : gnd    :                   :         :           :                
DRAM_ADDR[6]                 : N8        : output : 3.3-V LVTTL       :         : 3         : Y              
GPIO_1[14]                   : N9        : output : 3.3-V LVTTL       :         : 4         : Y              
GND                          : N10       : gnd    :                   :         :           :                
GPIO_1[15]                   : N11       : output : 3.3-V LVTTL       :         : 4         : Y              
GPIO_1[12]                   : N12       : output : 3.3-V LVTTL       :         : 4         : Y              
VCCD_PLL4                    : N13       : power  :                   : 1.2V    :           :                
GPIO_1[27]                   : N14       : output : 3.3-V LVTTL       :         : 5         : Y              
GPIO_1[24]                   : N15       : output : 3.3-V LVTTL       :         : 5         : Y              
GPIO_1[23]                   : N16       : output : 3.3-V LVTTL       :         : 5         : Y              
DRAM_ADDR[9]                 : P1        : output : 3.3-V LVTTL       :         : 2         : Y              
DRAM_ADDR[0]                 : P2        : output : 3.3-V LVTTL       :         : 2         : Y              
DRAM_DQ[13]                  : P3        : bidir  : 3.3-V LVTTL       :         : 3         : Y              
VCCIO3                       : P4        : power  :                   : 3.3V    : 3         :                
GND                          : P5        : gnd    :                   :         :           :                
DRAM_CS_N                    : P6        : output : 3.3-V LVTTL       :         : 3         : Y              
VCCIO3                       : P7        : power  :                   : 3.3V    : 3         :                
DRAM_ADDR[4]                 : P8        : output : 3.3-V LVTTL       :         : 3         : Y              
GPIO_1[13]                   : P9        : output : 3.3-V LVTTL       :         : 4         : Y              
VCCIO4                       : P10       : power  :                   : 3.3V    : 4         :                
GPIO_1[10]                   : P11       : output : 3.3-V LVTTL       :         : 4         : Y              
GND                          : P12       : gnd    :                   :         :           :                
VCCIO4                       : P13       : power  :                   : 3.3V    : 4         :                
GPIO_1[25]                   : P14       : output : 3.3-V LVTTL       :         : 4         : Y              
GPIO_1[20]                   : P15       : output : 3.3-V LVTTL       :         : 5         : Y              
GPIO_1[21]                   : P16       : output : 3.3-V LVTTL       :         : 5         : Y              
DRAM_ADDR[8]                 : R1        : output : 3.3-V LVTTL       :         : 2         : Y              
GND                          : R2        : gnd    :                   :         :           :                
DRAM_DQ[11]                  : R3        : bidir  : 3.3-V LVTTL       :         : 3         : Y              
DRAM_CLK                     : R4        : output : 3.3-V LVTTL       :         : 3         : Y              
DRAM_DQ[12]                  : R5        : bidir  : 3.3-V LVTTL       :         : 3         : Y              
DRAM_DQM[0]                  : R6        : output : 3.3-V LVTTL       :         : 3         : Y              
DRAM_DQ[7]                   : R7        : bidir  : 3.3-V LVTTL       :         : 3         : Y              
CLOCK_50                     : R8        : input  : 3.3-V LVTTL       :         : 3         : Y              
GND+                         : R9        :        :                   :         : 4         :                
GPIO_1[11]                   : R10       : output : 3.3-V LVTTL       :         : 4         : Y              
GPIO_1[9]                    : R11       : output : 3.3-V LVTTL       :         : 4         : Y              
GPIO_1[6]                    : R12       : output : 3.3-V LVTTL       :         : 4         : Y              
GPIO_1[4]                    : R13       : output : 3.3-V LVTTL       :         : 4         : Y              
GPIO_1[22]                   : R14       : output : 3.3-V LVTTL       :         : 4         : Y              
GND                          : R15       : gnd    :                   :         :           :                
GPIO_1[18]                   : R16       : output : 3.3-V LVTTL       :         : 5         : Y              
VCCIO3                       : T1        : power  :                   : 3.3V    : 3         :                
DRAM_DQ[9]                   : T2        : bidir  : 3.3-V LVTTL       :         : 3         : Y              
DRAM_DQ[10]                  : T3        : bidir  : 3.3-V LVTTL       :         : 3         : Y              
DRAM_DQ[8]                   : T4        : bidir  : 3.3-V LVTTL       :         : 3         : Y              
DRAM_DQM[1]                  : T5        : output : 3.3-V LVTTL       :         : 3         : Y              
DRAM_ADDR[7]                 : T6        : output : 3.3-V LVTTL       :         : 3         : Y              
DRAM_ADDR[5]                 : T7        : output : 3.3-V LVTTL       :         : 3         : Y              
SW[1]                        : T8        : input  : 3.3-V LVTTL       :         : 3         : Y              
GND+                         : T9        :        :                   :         : 4         :                
GPIO_1[8]                    : T10       : output : 3.3-V LVTTL       :         : 4         : Y              
GPIO_1[7]                    : T11       : output : 3.3-V LVTTL       :         : 4         : Y              
GPIO_1[5]                    : T12       : output : 3.3-V LVTTL       :         : 4         : Y              
GPIO_1[3]                    : T13       : output : 3.3-V LVTTL       :         : 4         : Y              
GPIO_1[2]                    : T14       : output : 3.3-V LVTTL       :         : 4         : Y              
GPIO_1[1]                    : T15       : output : 3.3-V LVTTL       :         : 4         : Y              
VCCIO4                       : T16       : power  :                   : 3.3V    : 4         :                
